**Foundation Repairs for Pinecrest Supports and Service Center**

**Location:**

Pinecrest Supports and Service Center

Building # 601/SO6924

575 Colwell Drive

Pineville, LA 71360

**Scope of Work:**

Contractor to provide all labor, materials, equipment, and tools necessary to lift and relevel of exterior and interior wall.

**Requirements:**

* Contractor shall remove approximately 50 feet of sidewalk on exterior of building in area to be repaired.
* Contractor shall install 10, 12 1/2 feet x 14 inch helical piers under wall and raise wall to as close to zero as possible.
* Contractor shall install two part urethane foam under interior walls to lift and pin foundation.
* Contractor shall reinstall concrete sidewalk. Sidewalk shall be approximately 50 feet long by 4 feet wide and 3 1/2 inch deep, with 3/8 inch steel rebar reinforcement and 3/8 inch by 6 inch dowel pins to old existing concrete.
* Contractor shall clean up any debris caused and or left behind and dispose of properly.

**Other Requirements:**

* Contractor shall coordinate with the assistant maintenance manager, Shannon T. Aymond at (318) 419-9786 to establish time and evacuation of work areas needed to complete the job.
* On-site visit required for all contractors submitting bids.
* Contactor shall supply a minimum 2 year warranty.
* Contractor shall supply own dumpster.