**Scope of Work:**

Contractor shall furnish all labor, tools, equipment, & materials to remove current roll up door units & replace with new roll up door units at the Raymond Laborde Correctional Center for the Louisiana Department of Corrections (DOC).

**Jobsite Location:**

Raymond Laborde Correctional Center

1630 Prison Road

Cottonport, LA 71327

**Job Specifications:**

-Contractor shall remove 19 existing roll up doors and guides located on the VoTech building. DOC shall be responsible for disposing of existing doors once removed.

-Contractor shall provide and install 19 new roll up doors and guides in the place of the doors that were removed.

**Door Specifications:**

* Door opening is 14' x 14'
* Heavy duty doors with 2" (51 mm) panel thickness
* 16-gauge steel intermediate and end stiles
* Ribbed steel exterior and 26-gauge steel back cover
* 20-gauge steel door exterior
* Standard 10,000 cycle springs
* Standard weather stripping
* Interior mounted slide locks
* Manually operated chain hoist
* Universal guides
* Color-Beige

Overhead Door Sectional Steel Doors Model 422 or equal

**Specify Brand/Model/Color of Door Bidding:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Planning & Scheduling:**

* Before entering the facility grounds to commence work, the contractor must check in with the maintenance department every day
* Work hours are to be 7:30 AM to 3:30 PM, Monday through Friday, unless approved by the Maintenance Manager James Desjardine

**Jobsite Visit Contact:**

James Desjardine james.desjardine@la.gov 318-876-4245

Josh Dauzat Joshua.dauzat@la.gov 318-876-4246